Intel Z77 chipset (Z77, LGA1155, DDR-III)  Mini-ITX Motherboard

AMI BIOS


A2290426.BIN  	BIOS for Z77, Nuvoton NCT6776F Super IO
		*** with Hardware Monitor 
		*** with STR (Suspend-To-RAM)
		*** with on-board LAN
		*** with 8-Ch HD Audio
		*** with Zotac Full Screen Logo


.64Mbit size 
.Support intel Ivy Bridge (22nm) Processors
.Initial mass production release
(March / 2012)

.64Mbit size
.2012/June update built
.Fixed compatibility issue with PCI-E (x1) cards
.Improved Memory Overclocking and XMP Profile support
.Show POST Error Message when CMOS Corrupted or Overclock failed
(June / 2012)

.64Mbit size
.2012/Nov update built
.Show UEFI RAID function group in Setup
.Hide some DVMT Pre-Allocated item
(November / 2012)

.64Mbit size
.2013/April update built
.Show CPU C3,C6,C7 Report and CPU Spread Spectrum in CPU Config
.Update CPU Microcode, VBIOS, RAID BIOS, LAN PXE ROM, ME Code 
.Added CPU VCore Offset Adjustment
.Changed Audio Codec ALC892 Verb table
(April / 2013)