Intel H87 chipset (H87, LGA1150, DDR-III)  Mini-ITX Motherboard

AMI BIOS


A2871211.BIN  	BIOS for H87, ITE8772E Super IO
		*** with Hardware Monitor 
		*** with STR (Suspend-To-RAM)
		*** with on-board LAN
		*** with 8-Ch HD Audio
		*** with Zotac Full Screen Logo


.64Mbit size 
.Support intel Haswell (22nm) Processors
.Initial mass production release
(May / 2013)

.64Mbit size 
.2013/June update built
.Updated CPU Microcode
.Corrected  Wake-On-LAN function (when LAN is disabled)
.Fixed "Setup Prompt Timeout" cannot load D4 after CMOS cleared
.Adjusted Display Config - Primary Display (Auto)
(June / 2013)

.64Mbit size 
.2013/July update built
.ME (Management Engine) code updated
.Corrected DP Audio issue
(July / 2013)

.64Mbit size 
.2013/December update built
.Updated CPU microcode table
.Updated Management Engine (ME) Code
.Updated VGA BIOS
.Corrected Smart Fan Speed after wakeup from S3
.Changed CMOS Setup (ZOTAC) background picture
(December / 2013)