AMD D3 Chipset (Hudson A75,  Socket FM2), DDR3, mITX Motherboard

AMI BIOS


A2340912.ROM 	BIOS for (AMD A75 + NCT5577 Super IO)
		* with Hardware Monitor 
		* with STR (Suspend-To-RAM)
		* with onboard LAN
		* with HD Audio
		* Zotac Full Screen Powerup Logo		

.32Mbit Flash
.2012/Oct built
.Initial Mass Production Release
(October / 2012)

.32Mbit Flash
.2012/Nov built
.Disabled Power button when flash BIOS
.Changed screen resolution to normal when boot to Shell.
.Fixed the issue no Windows Boot Manager after flash BIOS
(November / 2012)

.32Mbit Flash
.2013/Feb update
.Fixed warning message at POST, when using AMD "Richland" Processor.
(Feburary / 2013)

.32Mbit Flash
.2013/April update
.Fixed issue of Passwords can't be clear by CMOS jumper.
.Fixed SATA RAID function failure on previous BIOS
(April / 2013)

.32Mbit Flash
.2013/Sept update
.Added DDR3-2133MHz Memory Speed suport
.Changed CMOS Boot OS Selection (add Win7 UEFI)
(September / 2013)