Intel NM10 chipset (ATOM D510 / D525 , DDR-II) mDTX
AMI BIOS


I1222A.ROM  	BIOS for NM10, Nuvoton NCT5571D Super IO
		*** with Hardware Monitor 
		*** with STR (Suspend-To-RAM)
		*** with on-board LAN
		*** with 6-Ch HD Audio
		*** with Zotac Full Screen Logo


.8Mbit Flash size 
.Initial mass production release
(March/2010)

.8Mbit Flash size
.2010/Mid/March update built
.Fixed "Windows installation slow with some RAM" issue
(Mid/March/2010)

.8Mbit Flash size
.2010/End/March update
.Changed IDE Configuration settings
(End/March/2010)

.8Mbit Flash size
.2010/May update
.Suppressed Jmicron RAID Config ROM during bootup (use the CMOS Setup for RAID Config)
(May/2010)

.8Mbit Flash size
.2010/Dec update
.Corrected CMOS - CPU Temperature Reading issue
.Changed DMI content for "ZOTAC"
.Added support on new CPU variant model - ATOM D525
(Dec/2010)